Tender No:. 2026-27/Sports/2B/LNM-1481
The LNM Institute of Information Technology, Jaipur

TENDER NOTICE
The LNM Institute of Information Technology, Jaipur is a Deemed-to-be-University, set up as a Non-Profit Making institute engaged in imparting higher learning in Engineering, Technology and Science. We are located at Gram-Rupa Ki Nangal, Post-Sumel, Via-Jamdoli, Jaipur, Pin 302031 Rajasthan, under the joint venture of the Government of Rajasthan and Lakshmi & Usha Mittal Foundation.
The institute invites proposals from competent vendors for Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT. Bidders can submit their sealed offers/s at the following address by Email/Speed-Post/ Registered Post/ By-hand/courier before 05:00 PM on 31st  July, 2026.
Filing of Tender:
Option 1: Physical submission of offers (hard copy) in sealed envelopes.
Bids shall be addressed to the undersigned and deposited in the tender box available at the main gate of the institute in person/ Speed-Post/ Registered Post/ By-hand/courier of the Institute after marking due entries in the Receipt Book available with the Security Officer at the main gate. 
The tender subject and reference number must be mentioned on the envelope. 

Director
The LNM Institute of Information Technology,
Gram – Rupa Ki Nangal, Post – Sumel,
Via – Jamdoli, Jaipur- 302031

Option 2: Password-protected online submission via Email 
Password-protected offers can be submitted by the bidders via email at the below-mentioned email IDs.

tender-document@lnmiit.ac.in (password-protected document)
tender-password@lnmiit.ac.in (password only)
The tender subject and reference number must be mentioned in the subject line of the emails. 

Bid Process:
Technical & Commercial details on the company’s letterhead, duly signed and sealed by the authorized signatory, are required to be submitted in two separate envelopes/emails. 
Envelopes/Emails should be duly marked as follows: 
1. [bookmark: _Hlk219040947]Technical bid for the “Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT”. (Technical bid must be submitted without password protection)

2. [bookmark: _Hlk219038875][bookmark: _Hlk219040953]Commercial Bid for the “Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT” (The Commercial bid must be submitted with password protection.)
Both Envelopes/files should be enclosed/attached in a single envelope/email bearing the heading “Bid for the “Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT”) (Tender No. : 2026-27/Sports/2B/LNM-1481) ”. 
Note: The bidders/vendors are requested to go through the tender document carefully and ensure compliance with all specifications/instructions in this tender
Bids are liable to be rejected: 
· If the above-mentioned bid submission procedure is not followed.
· Incomplete and non-conforming bids.
· Arbitration: All disputes and differences arising between the two parties in connection with this order shall be mutually settled as far as possible, failing which, all such disputes shall be referred to arbitration and settlement under the provision of the Arbitration and Conciliation Act, 1996 and as amended from time to time or any such law for the time being prevailing in India. The venue of such arbitration shall be Jaipur.
Technical Bid: (in a separate sealed envelope/via email)

Bid for the Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT (Tender No. : 2026-27/Sports/2B/LNM-1481)

Bidder is required to furnish the requisite details as per the below mentioned table format and proof of such documents to be uploaded along with the bid under respective title/ headings as mentioned at column no ‘C’ accordingly.

	S.No.
	Title/ Heading
Details sought by buyer
	Details/ Certificate No. (Attached Y/N)

	A
	B
	C

	1.
	Bidder Firm Name & Registration No,
	

	2.
	Bidder’s Company profile or brief note
	

	3.
	PAN Card No,.
	

	4.
	GST Number
	

	5.
	List of Directors/ Partners/Proprietor/ Members of the Bidder’s Firm
	

	6.
	Detail of other associated/sister concerns (if any) of Directors/Partners/ Proprietor/ Members
	

	7.
	Bidder Turnover - Average annual turnover for last three years
	

	8.
	The Client List with some purchase orders and satisfactory certificate (to whom the vendor has delivered the goods/provided the services in the past (Three (03) purchase orders/work orders, at least one from each of the last three years, including the previous year.)
	

	9.
	If the bidder is authorized by the OEM/Manufacturer. Proof of the same is to be submitted with the Technical Bid
	

	10.
	An undertaking (self-certificate) that the agency has not been blacklisted by a Central/State/UT Government Institutions and there has been no litigation with any government department/institution on account of any services/supplies.
	

	11.
	Scanned copy of EMD/ Tender Fees paid through RTGS/NEFT (if required/asked in the tender)
	

	12
	Xerox copies of MoUs with previous colleges (minimum three) must be attached. (Applicable for student fest only).
	







Scope of Work
The successful bidder shall undertake the following work:
1. Supply and installation of Air-Cushion Free Floating Wooden Sports Flooring System.
2. Supply and application of Hard Plaster System to the squash court playing walls.
3. Supply and installation of Sound Board System.
4. Court line marking as per World Squash Federation (WSF) standards.
5. Final cleaning, testing, commissioning, and handing over of the completed court.

1. Technical Specifications
A. Air-Cushion Free Floating Wooden Sports Flooring System
The flooring system shall consist of a complete free-floating air-cushioned wooden sports flooring suitable for professional squash courts.

Surface Board
· Imported Kiln-Seasoned Maple Wood.
· Thickness: 21 mm.
· Width: 55–85 mm.
· Random lengths.
· Tongue and Groove profile.
· Finger-lock groove at board edges.
· Bottom side provided with air-pass grooves.
· Factory-finished sports flooring suitable for squash.
Under Frame
The under-frame shall consist of:
· Commercial quality Fir/Spruce/Pine timber runners.
· Runner Size: 70 mm × 45 mm.
· Anti-termite treated.
· EPDM air-cushion pads of 10 mm thickness fixed beneath runners.
· Pads fixed through both wings using corrosion-resistant nails.
· Runner spacing: 350 mm centre-to-centre.
Installation Method
· Existing IPS sub-floor shall be levelled before installation.
· A 600-micron polyethylene vapour barrier shall be laid over the entire floor.
· Timber runners shall be installed over the vapour barrier maintaining perfect level.
· Maple boards shall be screwed through the tongue only.
· Adjacent boards shall interlock through tongue-and-groove joints.
· Board ends shall be connected using wooden finger joints and approved adhesive.
· Expansion gap of 8–10 mm shall be maintained around the court perimeter.
· Flooring outside the glass back wall shall extend approximately 18 inches beyond the glass.
Area
· Internal Court Area: 672 Sq. Ft.
· Additional flooring behind glass wall: 35 Sq. Ft.
· Total Flooring Area: 707 Sq. Ft. (Approx.)
(Final quantity shall be measured at site.)

B. Hard Plaster System
The wall finish shall be specially designed for squash court applications.
System Description
The plaster system shall comprise:
· 12 mm Rubberized Gypsum Base Coat.
· 3 mm Fibre Reinforced Finish Coat.
· Total Thickness: Approximately 15 mm.
· Finished with high-quality washable sports-grade paint.
Minor variations in colour or micro surface checks due to drying characteristics shall not be considered defects and shall not affect performance.
Court Dimensions
Finished court dimensions between plaster faces shall be:
· Length: 9750 mm
· Width: 6400 mm
The client shall provide masonry walls that are plumb, level, square, and suitable for receiving the plaster system.

Area
Application shall be limited to:
· Front Wall
· Two Side Walls
Only the playing area below the red line shall receive the hard plaster system.
Approximate Area:
1060 Sq. Ft. Court
(Final quantity shall be measured at site.)

C. Sound Board System
The front wall shall be fitted with a professional squash sound board consisting of:
· 21 SWG Tin Sheet.
· Complete wooden support frame.
· Overall Height: 21 inches.
· Proper anchoring and finishing.
D. Toughened Glass Back Wall System
The bidder shall supply and install a complete international-standard glass back wall system including:
· Clear Toughened Safety Glass.
· Heavy-duty stainless steel fittings.
· Patch fittings.
· Glass connectors.
· Structural supports.
· Complete installation and alignment.
· All accessories required for a fully functional squash court.
The installed system shall comply with international squash court standards.

E. Court Line Marking
The bidder shall carry out complete game line marking in accordance with the latest World Squash Federation (WSF) specifications using approved sports marking paint.
2. Warranty
The successful bidder shall provide the following minimum warranties from the date of successful commissioning:
	Component
	Minimum Warranty

	Wooden Sports Flooring
	5 Years

	Hard Plaster System
	2 Years



Any manufacturing defect, installation defect, or workmanship defect occurring during the warranty period shall be rectified by the contractor at no additional cost to LNMIIT.

3. Eligibility Criteria
The bidder shall satisfy the following eligibility conditions:
1. The bidder shall be a manufacturer or authorized supplier of squash court systems.
2. Minimum 5 years of experience in the execution of squash court projects.
3. Successfully completed at least:
· Three similar squash court projects during the last five years.
4. The bidder shall submit satisfactory completion certificates/work orders from previous clients.
5. The bidder shall have adequate technical manpower and installation team.
6. The bidder shall not have been blacklisted by any Government Department, PSU, Autonomous Institution, University, or Educational Institution.
7. GST Registration, PAN, and all statutory registrations shall be mandatory.

5. Inspection and Acceptance
LNMIIT reserves the right to inspect the materials and workmanship during installation.
Final acceptance shall be based on:
· Compliance with technical specifications.
· Dimensional accuracy.
· Surface finish.
· Playing characteristics.
· Successful completion of installation.
· Submission of warranty documents.

6. Technical Summary
	Sr. No.
	Description
	Unit
	Approx. Quantity

	1
	Air-Cushion Free Floating Imported Maple Wooden Sports Flooring System
	Sq. Ft.
	707

	2
	Hard Plaster System including washable sports paint
	Sq. Ft.
	1060

	3
	Sound Board System complete with fittings
	Set
	1

	4
	Squash Court Game Line Marking
	Court
	1


The bidder shall quote unit rates, applicable taxes, installation charges, transportation charges, and total project cost separately.
7. Completion Period
The entire work shall be completed within 30 calendar days from the date of issue of the Work Order.
13. Right of the Institute
LNMIIT reserves the right to accept or reject any or all bids without assigning any reason and may modify the scope of work, quantities, or specifications in the interest of the Institute.



Technical specification: 
	
	Sr. No.
	Item Name
	Qty.
	UOM

	1
	Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT
	1
	 Nos


[bookmark: _Hlk214373706]

                                                                                                     Signature with seal





Annexure
To Whomsoever It May Concern
This is to confirm that we, the undersigned, intend to participate in Tender No. : 2026-27/Sports/2B/LNM-1481 for the tender/work titled: “Bid for the Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT”

We hereby certify the following:
No Conflict of Interest:
1. We declare that we have no conflict of interest in participating in the above tender. We further confirm that we are not engaged in any activity or association that may compromise, or be perceived to compromise, our impartiality or ability to fulfil the obligations of the tender.

Undertaking on Blacklisting & Litigation (Self-Certificate):
2. We hereby undertake that:
· Our agency/firm has never been blacklisted or debarred by any Central Government, State Government, Union Territory administration, or any other Institution/Organization.
· There is no ongoing or past litigation against our agency/firm with any Central Government, State Government, Union Territory administration, or any other Institution/Organization on account of any services/supplies.
· If at any stage the above declaration is found to be false, the Institute shall have the right to take any action as deemed appropriate, including rejection of our bid.

Site Visit /Understanding:
3. We confirm that we have visited the site/clearly understood the requirements and expectations of the college authorities.
Scope of Work:
4. We have thoroughly reviewed the scope of work mentioned in the bid document. The entire inventory/requirement/work has been verified and found to be in order. We also confirm that no additional items beyond the listed inventory/requirement will be required for successful completion of the work. However, if any additional item is required during execution, the same shall be provided by us as per the requirement.

Bidder Details

Name of Bidder: ______________________________________

Address: _____________________________________________

Contact Person: _______________________________________

Mobile No.: ___________________________________________

Email ID: _____________________________________________

Authorized Signatory: __________________________________

Signature & Stamp: ____________________________________


Date: _________________
Place: ________________


Commercial Bid: (in separate sealed envelope/password protected file via email)

Bid for the Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT
(Tender No. : 2026-27/Sports/2B/LNM-1481)

	S.No.
	Item Name/ Description
	Qty.
	UOM
	Rate
	Amount

	1.
	Supply, Installation, Testing and Commissioning of an International Standard Squash Court at LNMIIT
	1
	Nos.
	
	

	Total
	

	GST
	

	Total including GST
	



GENERAL TERMS AND CONDITIONS:
1. All applicable taxes such as GST must be clearly mentioned. If not specified, it shall be deemed that all such charges are included in the quoted price.
2. If the supplier does not have a particular item or proposes a different make than that specified in the tender, the same must be clearly highlighted in the bid.
3. Prices must be inclusive of all charges such as packing, forwarding, transit insurance, transportation, loading, unloading (up to 50 meters), installation, and any other incidental expenses.
4. Bid must be submitted on an F.O.R. basis for delivery at: The LNM Institute of Information Technology, Gram – Rupa Ki Nangal, Post – Sumel, Via – Jamdoli, Jaipur – 302031.
5. Bid shall remain valid for a minimum period of 60 days. No change in prices will be accepted during the validity period.
6. The LNMIIT reserves the right to reject any quotation without assigning any reason.
7. Payment terms shall be mutually decided and agreed upon between the Institute and the vendor.
8. The bidder must submit a No Conflict of Interest Declaration along with the bid.
9. The bid must be submitted on the company’s letterhead and in the LNMIIT-prescribed format only.
10. Any item or service not being supplied by the bidder must be clearly mentioned separately in the bid.
11. Vendors must provide a photocopy of their cheque/cancelled cheque along with the invoice for payment processing.
12. Prices shall be quoted in Indian Rupees (INR) only.
13. Total prices shall be quoted for the complete scope of work as per technical specifications, inclusive of all taxes, duties, insurance, packing, forwarding, and incidental charges.
14. Agencies or individuals who are debarred or blacklisted are not permitted to participate in the tendering process. Any agency engaging a debarred person for negotiations or representation is also liable to be debarred.
15. If the work is not completed within the stipulated time mentioned in the work order, the competent authority of LNMIIT reserves the right to accept partial work on suitable terms, cancel the supply/work order, withhold or stop payment, forfeit the Earnest Money Deposit, or debar the agency. The decision of the Competent Authority shall be final and binding.
16. In case two or more bidders quote the same rates, the final selection shall be made through a draw of lots conducted by a committee comprising LNMIIT administrative members(PCC).
17. Vendors are required to visit the site and conduct a detailed survey before submitting their bid to understand the exact requirements. No request for additional items or modifications will be entertained later.
18. A pre-bid meeting and/or site visit may be arranged prior to submission of bids to clarify any doubts regarding project details, scope of work, and required documents.



Signature with seal

